; Disks section 
;
; The Disks section identifies the disks in the device installation kit. 
; This section has the following format:
;
; diskN = "description",tagfile,directory
;

[Disks]
DVSTXRAIDX132 = "VIA StorX Driver Diskette X32 - XP", \XP\x86\VSTXRAID.TAG, \XP\x86
DVSTXRAIDX164 = "VIA StorX Driver Diskette X64 - XP", \XP\x64\VSTXRAID.TAG, \XP\x64
DVSTXRAIDX232 = "VIA StorX Driver Diskette X32 - SRV2003", \SRV2003\x86\VSTXRAID.TAG, \SRV2003\x86
DVSTXRAIDX264 = "VIA StorX Driver Diskette X64 - SRV2003", \SRV2003\x64\VSTXRAID.TAG, \SRV2003\x64
DVSTXRAIDX332 = "VIA StorX Driver Diskette X32 - VISTA", \VISTA\x86\VSTXRAID.TAG, \VISTA\x86
DVSTXRAIDX364 = "VIA StorX Driver Diskette X64 - VISTA", \VISTA\x64\VSTXRAID.TAG, \VISTA\x64
DVSTXRAIDX432 = "VIA StorX Driver Diskette X32 - WIN7", \WIN7\x86\VSTXRAID.TAG, \WIN7\x86
DVSTXRAIDX464 = "VIA StorX Driver Diskette X64 - WIN7", \WIN7\x64\VSTXRAID.TAG, \WIN7\x64
;
; Defaults section
;
; The Defaults section lists the default driver(s) for each hardware component supported by this file. 
; Setup highlights the default selection when it presents a list of drivers to the user.
;

[Defaults]
scsi = VSTXRAID_X132

;
; HwComponent Section
;
; A HwComponent section lists the drivers available for a particular component. 
; There is a HwComponent section for each type of component supported by the file.
;

[SCSI]
VSTXRAID_X132 = "VIA StorX Controller Series (Windows XP)"
VSTXRAID_X164 = "VIA StorX Controller Series (Windows XP - X64)"
VSTXRAID_X232 = "VIA StorX Controller Series (Windows SRV2003)"
VSTXRAID_X264 = "VIA StorX Controller Series (Windows SRV2003 - X64)"
VSTXRAID_X332 = "VIA StorX Controller Series (Windows VISTA)"
VSTXRAID_X364 = "VIA StorX Controller Series (Windows VISTA - X64)"
VSTXRAID_X432 = "VIA StorX Controller Series (Windows WIN7)"
VSTXRAID_X564 = "VIA StorX Controller Series (Windows WIN7 - X64)"
;
; Files.HwComponent.ID Section 
;
; A Files.HwComponent.ID section lists the files to be copied if the user selects a particular component option. 
; One of these sections must be present for each option listed in each HwComponent section.
;

[Files.SCSI.VSTXRAID_X132]
driver 	= DVSTXRAIDX132, VSTXRAID.sys, VSTXRAID
inf    	= DVSTXRAIDX132, VSTXRAID.inf
catalog = DVSTXRAIDX132, VSTXRAID.cat

[Files.SCSI.VSTXRAID_X164]
driver 	= DVSTXRAIDX164, VSTXRAID.sys, VSTXRAID
inf    	= DVSTXRAIDX164, VSTXRAID.inf
catalog = DVSTXRAIDX164, VSTXRAID.cat

[Files.SCSI.VSTXRAID_X232]
driver 	= DVSTXRAIDX232, VSTXRAID.sys, VSTXRAID
inf    	= DVSTXRAIDX232, VSTXRAID.inf
catalog = DVSTXRAIDX232, VSTXRAID.cat

[Files.SCSI.VSTXRAID_X264]
driver 	= DVSTXRAIDX264, VSTXRAID.sys, VSTXRAID
inf    	= DVSTXRAIDX264, VSTXRAID.inf
catalog = DVSTXRAIDX264, VSTXRAID.cat

[Files.SCSI.VSTXRAID_X332]
driver 	= DVSTXRAIDX332, VSTXRAID.sys, VSTXRAID
inf    	= DVSTXRAIDX332, VSTXRAID.inf
catalog = DVSTXRAIDX332, VSTXRAID.cat

[Files.SCSI.VSTXRAID_X364]
driver 	= DVSTXRAIDX364, VSTXRAID.sys, VSTXRAID
inf    	= DVSTXRAIDX364, VSTXRAID.inf
catalog = DVSTXRAIDX364, VSTXRAID.cat

[Files.SCSI.VSTXRAID_X432]
driver 	= DVSTXRAIDX432, VSTXRAID.sys, VSTXRAID
inf    	= DVSTXRAIDX432, VSTXRAID.inf
catalog = DVSTXRAIDX432, VSTXRAID.cat

[Files.SCSI.VSTXRAID_X464]
driver 	= DVSTXRAIDX464, VSTXRAID.sys, VSTXRAID
inf    	= DVSTXRAIDX464, VSTXRAID.inf
catalog = DVSTXRAIDX464, VSTXRAID.cat
;
; Config.DriverKey Section 
;
; A Config.DriverKey section specifies values to be set in the registry for particular component options. 
; Setup automatically creates the required values in the Services\DriverKey key. 
; Use this section to specify additional keys to be created under 
; Services\DriverKey and values under Services\DriverKey and Services\DriverKey\subkey_name.
;

[config.VSTXRAID]
value = "", EnableNcq, REG_DWORD, 0
;value = "", EnableRaid, REG_DWORD, 0
value = parameters\PnpInterface, 5, REG_DWORD, 1
value = "", DisableRaid, REG_DWORD, 0
value = "", DisableIdleDetection, REG_DWORD, 0
value = "", DisableGenRaidAwareness, REG_DWORD, 1
value = "", EnableRaidEmulation, REG_DWORD, 0
value = "", RaidEmulationType, REG_DWORD, 0
value = "", SectorNumberOfStrip, REG_DWORD, 64
value = "", CombineSequentialRwCmd, REG_DWORD, 1
value = "", DisableAtaDma, REG_DWORD, 0
value = "", DisableAtaMultiplePio, REG_DWORD, 0
value = "", DisableAtapiDma, REG_DWORD, 0
value = "", DisablePm, REG_DWORD, 4
value = "", DisableHotPlug, REG_DWORD, 0
value = "", MaxAtapiSrbTimeOutValue, REG_DWORD, 14
value = "", PreferedIpmMode, REG_DWORD, 0
value = "", PreferedIpmMethod, REG_DWORD, 0
value = "", IngoreBiosHipmSetting, REG_DWORD, 0
value = "", IngoreBiosHpIpmSetting, REG_DWORD, 0
value = "", HipmPartialPowerClock, REG_DWORD, 7
value = "", HipmSlumberPowerClock, REG_DWORD, 7
value = "", DisablePmDipm, REG_DWORD, 1
value = "", VSTXPnPPowerControl, REG_DWORD, 16

;
; HardwareIds.scsi.ID Section 
;
; A HardwareIds.scsi.ID section specifies the hardware IDs of the devices that 
; a particular mass storage driver supports. 
;

[HardwareIds.scsi.VSTXRAID_X132]
id = "PCI\VEN_1106&DEV_9040&CC_0104","VSTXRAID"
id = "PCI\VEN_1106&DEV_9041&CC_0104","VSTXRAID"

[HardwareIds.scsi.VSTXRAID_X164]
id = "PCI\VEN_1106&DEV_9040&CC_0104","VSTXRAID"
id = "PCI\VEN_1106&DEV_9041&CC_0104","VSTXRAID"

[HardwareIds.scsi.VSTXRAID_X232]
id = "PCI\VEN_1106&DEV_9040&CC_0104","VSTXRAID"
id = "PCI\VEN_1106&DEV_9041&CC_0104","VSTXRAID"

[HardwareIds.scsi.VSTXRAID_X264]
id = "PCI\VEN_1106&DEV_9040&CC_0104","VSTXRAID"
id = "PCI\VEN_1106&DEV_9041&CC_0104","VSTXRAID"

[HardwareIds.scsi.VSTXRAID_X332]
id = "PCI\VEN_1106&DEV_9040&CC_0104","VSTXRAID"
id = "PCI\VEN_1106&DEV_9041&CC_0104","VSTXRAID"

[HardwareIds.scsi.VSTXRAID_X364]
id = "PCI\VEN_1106&DEV_9040&CC_0104","VSTXRAID"
id = "PCI\VEN_1106&DEV_9041&CC_0104","VSTXRAID"

[HardwareIds.scsi.VSTXRAID_X432]
id = "PCI\VEN_1106&DEV_9040&CC_0104","VSTXRAID"
id = "PCI\VEN_1106&DEV_9041&CC_0104","VSTXRAID"

[HardwareIds.scsi.VSTXRAID_X464]
id = "PCI\VEN_1106&DEV_9040&CC_0104","VSTXRAID"
id = "PCI\VEN_1106&DEV_9041&CC_0104","VSTXRAID"
